            Light Pen Compatibility Guide
            =============================

CONTENTS
========

I. Introduction


II. 3270 Emulation

Attachmate EXTRA! for DOS 3270 Connectivity Software
DCA IRMA 3270 Adapters with E78 Plus and E78 Lite
EICON Access for DOS
IBM PC/3270 Emulation Program 3.0
3270 Emulation Software for Windows


III. Special Application Parameters and Options

Animator
AutoCAD
Colorgraphic Dual VGA+ Windows 3.0 Driver
The Controls Group
DESQview 2.0
DOSSHELL 4.0
Drafix CAD Ultra 4.01h
DrawPerfect 1.1
Dr. Halo III
Easel for DOS
EasyCAD 2.67
EGAPaint and ColoRIX
Fisher POS
GeoWorks Ensemble 1.0
GRiDPad Applications
IBM CAD 1.2, 1.2.1
Knowledge Pro for DOS
MapInfo 4.50
MetaWindows 3.7
NIDA Corp. Applications
Norton Utilities 6.0
Paintbrush 4.0
PC Paintbrush IV and PC Paintbrush IV Plus 1.0
PC Tools 7.0
Splash 1.0
Storyboard Plus 2.0
TEMPRA Pro 1.03
TEMPRA 2.01 for Hercules Graphics Station Card
TIGA High Resolution
WordPerfect for DOS 5.1
WordPerfect for DOS 6.0


IV. Applications Compatibile with FTG Light Pens

===============================================================



I. Introduction
===============

This guide lists usage notes for a variety of software packages
that require special handling to work properly with FTG light
pens.

Some applications require special options to be set within the
programs themselves. Others may also require parameters to be
set in the light pen software. These options and parameters are
explained here.

We start with IBM 3270 emulation applications then
alphabetically list additional DOS applications.

The MouseTrap function of PXL-BIOS must be enabled when running
the applications in Section II that are marked with a star (*).
See the section on MouseTrap in the PXL Interface User's Guide
for additional information about MouseTrap.

FTG is continually adding to and updating this list.

A list of applications that have been tested with FTG light
pens and interfaces completes this guide.



II. 3270 Emulation
==================

Attachmate EXTRA! for DOS 3270 Connectivity Software
----------------------------------------------------
FTG Light Pens are supported by Attachmate's EXTRA! for DOS
3270 Connectivity Software when using a variety of COAX and
Local Area Network Adapters.

To enable the light pen in EXTRA! for DOS:

1. Run the customization program by changing to your EXTRA!
   subdirectory and typing "config" at the DOS prompt.

2. Select the ADVANCED FEATURES field from the Main Selection
   Menu.

3. Highlight the field next to the Light Pen feature in the Screen
   section.

4. Press the Space bar to change the field to Yes.

Optionally you may load light pen support each time you start
EXTRA! by typing "extra -lp" then press Enter.

Consult the EXTRA! documentation for more information.

                                                                    
DCA IRMA 3270 Adapters with E78 Plus and E78 Lite
-------------------------------------------------
All the PXL Light Pen Interfaces have been successfully tested
with DCA's IRMA 3270 Emulation adapters and E78 Plus and E78
Lite emulation software.

To use the light pen with E78 Plus you must first enable the
light pen function in the E78GEN configuration program. After
executing E78GEN, select the PC OPTIONS menu item. Select the 0
(zero) choice from the list of choices for LIGHT PEN.

E78 Plus supports the light pen when using most display
adapters. If you experience problems using the light pen in a
host application, run the E78GEN program and select GENERAL
PURPOSE for Display Adapter from the DISPLAY options menu.
Retry the light pen in the host application.

To enable the light pen in E78 Lite add the "/I=0" command line
option when you run LE78.EXE. Type "le78 /i=0" to run E78 Lite
with a light pen.

Consult your E78 Plus or E78 Lite documentation for more infor-
mation.

NOTE 1: All releases of the original E78 (before the Plus was
added) and releases earlier than 1.1.0 of E78 Plus software do
not support the PXL Light Pen Interfaces. Contact DCA customer
support at (800) 631-4171 for update information.

NOTE 2: The IBM PS/2 Model 70 only has three expansion slots:
one 16-bit slot with the special video extension and two 32-bit
slots. The Irma 2-MCA will not fit into a 32-bit slot so it
must be plugged into the 16-bit/video extension slot. The
PXL-480 will work in either of the 32-bit slots but requires
the optional S-215B External Sync Cable to operate. Please
contact your dealer to order this cable.

NOTE 3: The 1.4.0 release of E78 Plus is incompatible with the
MouseTrap mouse emulation function of PXL-BIOS. Don't enable
MouseTrap when running the PXLSETUP program. Contact FTG
Customer Support for more information.

                                                                    
EICON Access for DOS
--------------------
FTG is now marketing FT-3270 Light Pen Support Program to
support the AccessAPI of EICON's Access for DOS. This program
adds light pen support to Access for DOS which does not
otherwise support light pens directly. Contact your FTG dealer
to purchase FT-3270 if you are using Access for DOS.

                                                                    
IBM PC/3270 Emulation Program
-----------------------------
FTG now markets FT-3270 Light Pen Support Program to support
IBM PC/3270 Emulation Software throught EHLLAPI. This
program adds light pen support to PC/3270 3.0 in Full-Function
DOS mode which does not otherwise support light pens directly.
Contact your FTG dealer to purchase FT-3270 if you are using
PC/3270.

                                                                    
3270 Emulation Software for Windows
-----------------------------------
Most 3270 emulation software packages designed to work in the
Windows environment issue the 3270 light pen select function
when you press the right mouse button. To simulate a right
mouse button press with the pen hold the Alt key down and press
the pen to the screen. You can also issue a light pen select
function by first pressing the R box on the LPNBTNS PEN icon,
then pressing the pen to the screen to make your selection.

You can also use the Pen Button Action options in the Windows
Light Pen Control Panel to customize the pen to work with
specific 3270 emulation software for Windows.

You should find that checking the Disable Drag checkbox in
the Windows Light Pen Control Panel will provide better
accuracy when using Attachmate EXTRA! for Windows.

Contact the publisher of your Windows 3270 software for
additional information.


                                                                    
III. Special Application Parameters and Options
===============================================

FTG's MouseTrap mouse emulation function allows light pen input
with most applications supported by a Microsoft Mouse.
MouseTrap must be enabled in the PXLSETUP program to run all of
the following applications marked with a star (*).

                                                                    
Animator (*)
--------
Type "pxl-bios a4" then press Enter at the DOS prompt to set up
special processing for AutoDesk Animator.

Configure Animator for a Microsoft Mouse.

                                                                    
AutoCAD (*)
-------
The ADI interface that Autodesk provides for 3rd-party pointing
devices was optimized for a digitizer. Special translation
factors are required by PXL-BIOS to properly emulate a
digitizer, and these factors change with release level, display
adapter and on-screen options (menus, status line, etc.)

FTG has determined these factors for a number of popular
configurations and encoded them into the FTG-ADI.DTA file.
PXLSETUP will read this file and build the parameters that are
appropriate for your configuration into PXL-BIOS.

To prepare your AutoCAD system to work with the Light Pen you
will need to complete the following steps.

1. Rerun PXLSETUP. Select Yes when PXLSETUP asks whether you'll be
   using AutoCAD.

2. PXLSETUP then provides an option menu with a list of different
   version/display configurations. Choose the monitor type and
   version of AutoCAD you will be using.

3. Run AutoCAD and change the input device configuration.  Choose
   the ADI digitizer (2) and use the default interrupt parameter
   (79h).

                                                                    
Colorgraphic Dual VGA+ Windows 3.0 Driver
-----------------------------------------
Type "pxl-bios a22" then press Enter at the DOS prompt to set up
special processing for the Windows 3.0 driver for the
Colorgraphic Dual VGA+. This display adapter allows the Windows
desktop to cover two seperate VGA monitors.

                                                                    
The Controls Group (*)
------------------
Type "pxl-bios a18" then press Enter at the DOS prompt to set up
special processing for The Controls Group refrigeration control
systems applications.

                                                                    
DESQview 2.0 (*)
------------
Type "pxl-bios a11" and press Enter at the DOS prompt to set up
special processing for Quarterdeck's DESQview.

Configure DESQview for a Microsoft Mouse.

                                                                    
DOSSHELL 4.0 (*)
------------
Type "pxl-bios a7" and press Enter at the DOS prompt to set up
special processing for IBM's DOSSHELL 4.0.  The example below
shows what the file DOSSHELL.BAT should look like.  Use a DOS
text editor or a word processor capable of exporting DOS text
to delete the underlined section.

@C:
@CD C:\DOS
@SHELLB DOSSHELL
@ IF ERRORLEVEL 255 GOTO END
:COMMON
@BREAK=OFF
@SHELLC/MOS:PCIBMDRV.MOS/TRAN/COLOR/DOS/
       -----------------
MENU/MUL/SND/MEU:SHELL.MEU/CLR:SHELL.CLR/
PROMPT/MAINT/EXIT/SWAP/DATE
:END
@BREAK=ON

                                                                    
Drafix CAD Ultra 4.01h (*)
----------------------
Type "pxl-bios a13 f1 k1" and press Enter at the DOS prompt to
set up special processing for Drafix CAD Ultra 4.01h Dec 90
before running the DFXSETUP program to install or reinstall
Drafix.

Select Microsoft Mouse for the pointing device in DFXSETUP.

                                                                    
DrawPerfect 1.1 (*)
---------------
Type "pxl-bios a10" and press Enter at the DOS prompt to set up
special processing for WordPerfect Corporation's DrawPerfect
1.1.

Configure DrawPerfect for a Microsoft Mouse.

To allow the Light Pen to function correctly with the
WordPerfect Shell using DrawPerfect and WordPerfect follow
instructions for WordPerfect 5.1.

                                                                    
Dr. Halo III
------------
Follow these steps if you are using Dr. HALO III from Media
Cybernetics:

1. Type "pxl-bios f1 k1" and press Enter. This will flood the screen
   background with blue and keep the background flooded.

2. Create a work copy of Dr. HALO III by following the
   instructions provided with that package. Run the Dr. HALO
   Setup program and select KEYBOARD as the pointing device.
   NOTE: You may find light pen responsiveness somewhat improved
   if you do not enable the on-screen coordinate display.

3. DO NOT run the INIT.BAT program as instructed in the Dr. HALO
   III manual. Instead, copy HALOFTGI.COM from the Advanced PXL
   Support Software Diskette to your Dr. HALO III work disk or
   directory.

4. Use an ASCII editor such as Wordstar (in non-document mode) or
   EDLIN to edit the INIT.BAT file to replace the line that
   reads:

      HALOKBDI -i[n] (where [n] is an integer parameter)

   with a new line that says:

      HALOFTGI -i[n] ([n] must be the same integer parameter)

   NOTE:  The "-i[n]" parameter may not be included in your
   INIT.BAT file. If your INIT.BAT has the line:

      HALOKBDI       (without the "-i[n]" parameter)

   replace the line with:

      HALOFTGI       (without the "-i[n]" parameter)

5. Type "init" then press Enter to run the edited version of the
   INIT.BAT file. This will configure Dr. HALO III to use a
   light pen rather than the keyboard as the pointing device.

6. Type "drhalo" then press Enter to run Dr. HALO III. If light pen
   offset errors occur, you will need to lock PXL-BIOS into the
   display mode used. See the Software chapter in the User's
   Guide for more information.

NOTE: HALOFTGI has been provided by special arrangement with
Media Cybernetics, and it is extremely important that all light
pen support questions be directed to FTG rather than Media
Cybernetics. Please do not call Media Cybernetics with any
light pen questions. FTG may be reached toll-free at
1-800-962-3900. Thank you for your cooperation in this matter.

                                                                    
Easel for DOS (*)
-------------
Type "pxl-bios a1" and press Enter at the DOS prompt to set up
special processing for Interactive Images' Easel.

Configure Easel for a Microsoft Mouse.

                                                                    
EasyCAD 2.67 (*)
------------
Type "pxl-bios a23" and press Enter at the DOS prompt to set up
special processing for Evolution Computing's EasyCAD.

                                                                    
EGAPaint and ColoRIX
--------------------
Follow these steps if you are using EGAPAINT or COLORIX from
RIX Softworks:

1. Type "pxl-bios f1 k1 a20" and press Enter. This will flood the
   screen background with blue, keep the background flooded, and
   set up special processing for ColoRIX.

2. Create a work copy of EGAPAINT or COLORIX by following the
   instructions provided with that package. Run the EGASETUP or
   VGASETUP program and select FTG LIGHT PEN as the input device
   type. For setting INITIAL CONDITIONS:

   a. Select Hold Button to Draw and then confirm by pressing
   the Enter key.

   b. Highlight Menu Key Select and confirm by pressing the
   Enter key.

   c. Highlight Menu Key Select Enabled and press the Enter
   key.

   d. Save this configuration and exit.

3. Use an ASCII editor such as WordStar (in non-document mode) or
   EDLIN to edit the appropriate configuration file as follows:

   - In EGAPAINT.CFG, the line beginning #M should
     read:  #M 6123 0280 015D 0000 0000

   - In COLORIX.CFG, the line beginning #M should
     read:  #M 6123 0280 01DF 0000 0000

4. Type "egapaint" or "colorix" then press Enter to run the program.
   If light pen offset errors occur, you will need to lock PXL-
   BIOS into the display mode used. See the Software chapter in
   the User's Guide for more information.

                                                                    
Fisher POS (*)
----------
Type "pxl-bios a16" then press Enter at the DOS prompt to set up
special processing for Fisher Business Systems point of sale
applications.

                                                                    
GeoWorks Ensemble 1.0 (*)
---------------------
Special PXL-BIOS command line options may be necessary when
using GeoWorks Ensemble 1.0.

Run GEOS.EXE and select Professional, Preferences, Mouse from
the icon based menus. Change the Type of mouse to "Nothing else
works", then enter OK. Next adjust the Mouse Acceleration to
Slow, then enter OK. This should enable the pen to function
correctly, you may have to move the pen on and off the screen
at startup to aline the cursor. You may also have to lock the
video mode to the resolution you are using under Ensemble with
PXL-BIOS L mode. Refer to the Software chapter in the User's
Guide for more information.

                                                                    
GRiDPad Applications (*)
--------------------
Type "pxl-bios a6" and press Enter at the DOS prompt to set up
special processing for GRiD Systems' GRiDPad applications using
the desktop PC drivers for VGA included with the GRiDPen Pro
gram Development Kit.

                                                                    
IBM CAD 1.2, 1.2.1 (*)
------------------
Type "pxl-bios a21" then press Enter at the DOS prompt to set up
special processing for IBM CAD.

                                                                    
Knowledge Pro for DOS (*)
---------------------
Type "pxl-bios a19" then press Enter at the DOS prompt to set up
special processing for Knowledge Pro for DOS graphic
applications.

                                                                    
MapInfo 4.50 (*)
------------
There are different PXL-BIOS configurations for the VGA and for
the EGA. If you are using a VGA type "pxl-bios a15 f4 k1" and
press Enter at the DOS prompt; if you are using an EGA type "pxl-
bios a15 f1 k1" and press Enter at the DOS prompt to set up
special processing and blue background flood for MapInfo 4.50.

Configure MapInfo 4.50 for a Microsoft Mouse on the Default
port.

There is neither mouse nor light pen control in the Main Menu.
The light pen is, however, fully functional in the Mapping
menu.

                                                                    
MetaWindows 3.7 (*)
---------------
Type "pxl-bios a2" and press Enter at the DOS prompt to set up
special processing for Metagraphics Software's MetaWindows.

Configure MetaWindows for a Microsoft Mouse.

                                                                    
NIDA Corp. Applications (*)
-----------------------
Type "pxl-bios a12" and press Enter at the DOS prompt to set up
special processing for NIDA Corporation instructional
applications.

Configure the NIDA application for a Microsoft Mouse.

                                                                    
Norton Utilities 6.0 (*)
--------------------
Special PXL-BIOS command line options are not necessary when
using Norton Utilities 6.0.

Run NORTON.EXE and select Video and Mouse Options... from the
Configure menu.  Change the Graphics Option to Standard then
select Save to configure Norton Utilities for a light pen.

                                                                    
Paintbrush 4.0 (*)
--------------
Type "pxl-bios a5" and press Enter at the DOS prompt to set up
special processing for Microsoft's Paintbrush 4.0.

                                                                    
PC Paintbrush IV and PC Paintbrush IV Plus 1.0 (*)
----------------------------------------------
Type "pxl-bios a9" and press Enter at the DOS prompt to set up
special processing for Zsoft's PC Paintbrush IV and PC
Paintbrush IV Plus Version 1.0.

Configure PC Paintbrush for a Microsoft Mouse.

                                                                    
PC Tools 7.0 (*)
------------
Special PXL-BIOS command line options are not necessary when
using PC Tools 7.0.

Run PCCONFIG.EXE from the PCTOOLS directory, choose Mouse,
change the Graphics Mouse Option to off then select OK to
configure, exit, and save. This operation will now allow PC
Tools to operate with a light pen.

                                                                    
Splash 1.0 (*)
----------
Type "pxl-bios a3" then press Enter at the DOS prompt to set up
special processing for Spinnaker's Splash.

Configure Splash for a Microsoft Mouse.

                                                                    
Storyboard Plus 2.0 (*)
-------------------
Type "pxl-bios a6" and press Enter at the DOS prompt to provide
special processing for IBM's Storyboard Plus Version 2.0.

Run Storyboard Plus. At the Storyboard Plus main menu choose
Setup. Choose Other as the input device. Do not select
Microsoft or any other Mouse.

                                                                    
TEMPRA Pro 1.03 (*)
---------------
Type "pxl-bios a24" and press Enter at the DOS prompt to provide
special processing for Mathematica's TEMPRA Pro.

                                                                    
TEMPRA 2.01 for Hercules Graphics Station Card (*)
----------------------------------------------
Type "pxl-bios a14 l#n" (where n is the user mode number assigned
to the TIGA mode to be used in TEMPRA) and press Enter at the
DOS prompt to set up special processing for Mathematica's
TEMPRA Demo 2.01 included with the Hercules Graphics Station
Card.

TEMPRA is automatically configured for a Microsoft Mouse. Use
the pen's switch alone to access TEMPRA Button 1 functions.
Hold the Ctrl key down and push the pen to the screen to
activate TEMPRA Button 2 functions.

The full graphics screen scrolling, that occurs when canvases
are set larger than the actual screen resolution, will cause
pen cursor offsets. The Zoom box uses relative light pen
movements for positioning.

                                                                    
TIGA High Resolution
--------------------
Type "pxl-bios a17" and press Enter at the DOS prompt to set up
special processing to suppress excessive jitter for TIGA
operating in resolutions greater than 1024 X 768.

                                                                    
WordPerfect for DOS 5.1 (*)
-----------------------
Type "pxl-bios a10" and press Enter at the DOS prompt to set up
special processing for WordPerfect Corporation's WordPerfect
5.1. Follow these instructions to configure WordPerfect 5.1:

1. Start WordPerfect.

2. Press SHIFT+F1 to display the Setup menu.

3. Press 1 to choose Mouse.

4. Press 5 to choose Acceleration Factor.

5. Press 1 to set the mouse acceleration factor to 1.

6. Press ENTER three times to save these new values.

WordPerfect is now configured for a light pen.

                                                                    
WordPerfect for DOS 6.0 (*)
-----------------------
A new mouse driver is included with WordPerfect 6.0 that
supports absolute/pen devices directly through the mouse
interface. Follow these instructions to configure WordPerfect
6.0 for this driver:

1. Start WordPerfect.

2. Press SHIFT+F1 to display the Setup menu.

3. Press 1 to choose Mouse.

4. Press 1 to choose Type.

5. Select Mouse Driver (Absolute/Pen) from the list and select OK.

6. Select Close.

7. Exit then restart WordPerfect to start using the pen.


IV. Applications Compatibile with FTG Light Pens
================================================

This section lists some of the many software products
compatible with FTG's light pens and the vendors who sell these
products. In addition to the applications listed, FTG light pen
products support all Microsoft Windows, Windows NT and IBM OS/2
compatible applications. All applications, except those marked with
an asterisk (*), require a PXL Light Pen Interface. With the number
of new software products entering the market every day, your
application may not be listed please call FTG at 1-800-962-3900
to find out if it is supported.

Authoring
---------
Quest*
Allen Communications
(801) 537-7800

Communications
--------------
EMU-TEK
FTG Data Systems
(800) 962-3900

RCOM-2/PC*
Computer Vectors Inc.
(800) 262-RCOM

Computer-Aided Design
---------------------
AutoCad 
Autodesk, Inc.
(415) 332-2344

CADKEY 
Micro Control Systems
(203) 647-0220

CADvance 
Calcomp
(714) 821-2438

Design Board Professional 
Mega Cadd Inc.
(206) 623-6245

Drafix CAD Ultra 
Foresight Resources Corp.
(800) 231-8574

EasyCAD 
Evolution Computing
(602) 967-8633

FastCAD 
Evolution Computing
(602) 967-8633

IBM CAD
IBM Corp.
(407) 982-1975

ProDesign II 
American Small Business Computers
(918) 825-4844

DataBase
--------
FoxPro
Microsoft
(206) 882-8080

Paradox
Borland International
(408) 438-8400

DBase
Borland International
(408) 438-8400

Desktop Publishing
------------------
Artline
Digital Research
(404) 646-6464

First Publisher 
Software Publishing Corp.
(415) 962-8910

FONTASY 
Prosoft
(818) 765-4444

Iprint
Indigo Software, Ltd.
(613) 728-0016

Publisher's Paintbrush 
ZSoft Corporation
(404) 428-0008

Ventura Publisher 
Xerox Corp.
(800) 822-8221

Engineering
-----------
HiWIRE 
Wintek Corp.
(800) 742-6809

Graphics
--------
Animator 
Autodesk, Inc.
(415) 332-2344

AutoSketch 
Autodesk, Inc.
(415) 332-2344

ColoRIX VGA Paint 
RIX Softworks 
(714) 476-8266

Drawing Tablet II 
K Software House, Inc.
(615) 294-5090

DR. Halo III
Media Cybernetics
(800) 446-HALO

EGAPaint 
RIX Softworks
(714) 476-8266

FANTAVISION 
Broderbund Software. Inc.
(800) 527-6263

PC Paintbrush
ZSoft Corporation
(404) 428-0008

Splash 
Spinnaker Software
(617) 494-1200

Television 
LCS Telegraphics
(800) 437-0036

IBM 3270 Terminal Emulation
---------------------------
Access for DOS (Requires FTG FT-3270 Product)
EICON Technology
(514) 631-2592

Datasync*
CLEO Communication
(313) 662-2002

Dynacomm*
Network Software Associates
(714) 768-4013

EXTRA!*
Attachmate Corp.
(800) 426-6283

Irma / E78 Plus*
Digital Communications Assoc.
(404) 442-4000

IRMAX*
Digital Communications Assoc.
(404) 442-4000

LinkUp*
Chi Corporation
(800) 431-3460

pcPATH SNA 3270*
ICOT Corporation
(800) 434-0515

PC/3270 (Requires FTG FT-3270 Product)
IBM Corp
(407) 982-1975

Netware 3270*
Novell, Inc.
(800) 453-1267

RabbitSTATION Coax*
Productivity Technology
(215) 630-4530

SNA Exchange*
Passport Communications
(512) 328-9830

Intergrated
-----------
Microsoft Works 
Microsoft
(206) 882-8080

First Choice 
Software Publishing Corp.
(415) 962-8910

Mapping Information Systems
---------------------------
MapEdit 
Strategic Locations Planning, Inc.
(408) 985-7400

MapInfo 
Mapinfo Corp.
(518) 274-8673

Online Services
---------------
CompuServe Information Manager
CompuServe
(614) 457-8600

Prodigy 
Prodigy Services Co.
(914) 993-8000

Operating Environments
----------------------
DESQview 
Quarterdeck Office Systems
(800) 845-6621

GeoWorks Ensemble 1.0
GeoWorks
(414) 644-3456

GEM 
Digital Research, Inc.
(408) 649-3896

HP New Wave
Hewlett Packard
(800) 848-9283

Windows and Windows NT (Optional Windows NT Drivers Available)
Microsoft Corp.
(206) 882-8080

OS/2 (Optional OS/2 Drivers Available)
IBM Corp.
(407) 982-1975

Pen Computing
-------------
Microsoft Pen Extensions for Windows
Microsoft Corp.
(206) 882-8080

PenDOS
CIC
(415) 802-7777

PenRight! Pro
GRiD Systems
(415)656-4700

Presentation Graphics
---------------------
35MM Express 
Businness & Professional Software Inc.
(617) 494-1155

Applause II 1.0 
Aston Tate
(213) 329-8000

Image Builder 
Communications Dynamics, Inc.
(503) 684-5151

Presentation Team 
Digital Reserarch Inc.
(408) 649-3896

Storyboard 2.0 
IBM Corp.
(407) 982-1975

VP-Graphics 
Paperback Software Intel
(415) 644-2116

Productivity
------------
Project Scheduler Network 
Scitor Corp.
(415) 570-7700

Programming
-----------
Microsoft QuickC 
Microsoft Corp.
(206) 882-8080

Microsoft QuickBASIC 
Microsoft Corp.
(206) 882-8080

Spreadsheet
-----------
Lotus 1-2-3 2.3 
Lotus Development
(617) 577-8500

Lotus 1-2-3 3.1 
Lotus Development
(617) 577-8500

Quattro Pro 
Borland International
(408) 438-8400

Utilities
---------
Control Room 
Ashton-Tate
(213) 329-8000

Direct Access 5.0 
Fifth Generation Systems
(504) 291-7221

DOS Shell 
Microsoft
(206) 882-8080

DOS Shell 
IBM Corp.
(407) 982-1975 

Norton Utilities 5.0 
Symantec Corp.
(408) 253-9600

PC Tools Deluxe 6.0 
Central Point Software
(503) 690-8088

Xtree Gold 2.0 
Xtree Company
(805) 541-0604

Vertical Applications
---------------------
ChemCad 
C-graph
(512) 459-3562

Computerized Sensory Analysis
Compusense
(519) 836-9993

Final III
Davies & Assoc.
(502) 582-2214

Knowledge Pro DOS 
Knowledge Garden Inc. 
(518) 766-3000

Mitchell On Demand
Mitchell International
(619) 758-6550

PASS
Select Ticketing Systems
(315) 479-6663

Word Processing
---------------
Word 5.0 
Microsoft
(206) 882-8080

WordPerfect
WordPerfect
(801) 226-6800


----------------------------------------------------------------

Copyright (C) 1995 FTG Data Systems. All rights reserved.

Revised 5/19/95

----------------------------------------------------------------