$OS
DOS
$GENERIC
d_isdasd.dt
$FILENAME
d_isdasd.dt
$DESCRIP
DASD Device Table
$SHORT
DASD
$VERSION
2
$CLASS
device
$IN_ATTRIBUTE
WRITE
READ
BLOCK
$DEVICE_TYPE
80
$CONTROL_BYTE
40
$DD_ATTRIBUTE
0
$SCSI_ID
0-7
$LUN
0-1
$SCAN
4
0
/T30/D10
$IDENTIFY
inquiry(20)
noerror
00 = 00
#if the manufacture string is null fail (alpha drive ??)
08 ~ 0
#if the product string ends with a *F it is a floptical, so fail also
1E ~ 2a
1F ~ 46
$DRIVE_LETTER

